{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Titul_Vstupy","Vystupy","Sheet3"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Titul_Vstupy","index":0,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
[" Program Flood_V:  "]
["           Vývoj:"]
["                 Fakulta životního prostredí"]
["                 Ceská zemedelská universita v Praze "]
["                 Katedra biotechnických úprav krajiny KBUK ad."]
["                 Rešitelé: Pavel Kovár, Jiri Zezulák"]
["           Metoda:"]
["                 Program vypocte objem a prubeh návrhových povodnových vln"]
["                 proporcionálne s TUH, dle návrhových prutoku CHMU"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Vstupy programu pro pripadovou studii Zarošice a Scénár Q-N:"]
["Lokalita:","Cname=","Zarošice"]
["Scénár:","Ename=","Q-N"]
["Adresár:","Fname=","c:\\temp"]
["Plocha povodí:","Area=",0.18,"(km2)"]
["Délka hlavního toku (udolnice):","L=",790,"(m)"]
["Prumerný sklon udolnice:","Y=",7.3,"(%)"]
["Cislo odtokové krivky CN:","CN=",73,"(-)"]
["Cislo max. odtokové krivky CNM:","CNM=",87,"(-)"]
["Pocátecní bezodtok. retence:","Reten=",0,"(mm)"]
[]
["Pocet poradnic zadaného hydrogramu:","II=",30,"(-)"]
["Délka casového kroku:","Delt=",0.5,"(hod)"]
["Doba opakování, Qmax:","Qu, Qmax=","(roky)","(m3/s)"]
[null,null,1,0.06]
[null,null,2,0.14000000000000001]
[null,null,5,0.3]
[null,null,10,0.49]
[null,null,20,0.75]
[null,null,50,1.2]
[null,null,100,1.7]

{"sheet":"Vystupy","index":1,"n_rows":76,"n_cols":19,"rows_kept":76,"cut":false,"hidden":false,"merged":[]}
["Výstupy procedury Flood_V pro pripadovou studii ZarošiceQ-N:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chybová sdelení a výstrahy"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"casovy krok > 0.25*Tk -> moznost oscilace TUH pri vypoctu Qmax: 1-letá voda"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"casovy krok > 0.25*Tk -> moznost oscilace TUH pri vypoctu Qmax: 2-letá voda"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"casovy krok > 0.25*Tk -> moznost oscilace TUH pri vypoctu Qmax: 5-letá voda"]
[]
[]
[]
[]
[]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)",null,null,null,null,null,null,"index","cas","Q1","Q2","Q5","Q10","Q20","Q50","Q100"]
["Cetnost opakování:","N=",1,"(let)",null,null,null,null,"(-)","(hod)","(m3/s)","(m3/s)","(m3/s","(m3/s)","(m3/s)","(m3/s)","(m3/s)"]
["Hodnota kulminace (dle CHMU):","Qmax=",0.06,"(m3/s)",null,null,null,null,1,0.5,7.7817033773601805E-3,1.7630519626892573E-2,4.0309331473203563E-2,6.6175294111654681E-2,9.3481057708331136E-2,0.14666321975856336,0.21111459408646088]
["Poradnice doby kulminace","IMAX=",4,"(-)",null,null,null,null,2,1,1.4962426234864924E-2,2.9879912028214824E-2,5.3611602561648354E-2,6.9908955245604545E-2,9.3481057708331136E-2,0.14666321975856336,0.21111459408646088]
["Doba dobihani:","TL=",1.5023150587717058,"(hod)",null,null,null,null,3,1.5,4.2445636629027714E-2,8.9208263390051043E-2,0.18510692351207408,0.2896879694908564,0.36886186056396159,0.48325039391198399,0.62691042688332921]
["Objem vlny:","VOL=",0.46144210501369126,"(tis. m3)",null,null,null,null,4,2,5.9999999999999991E-2,0.14000000000000001,0.3,0.43897349209849701,0.56392352066063034,0.83409207459416956,1.1641793419929285]
[null,null,null,null,null,null,null,null,5,2.5,4.3580643251293065E-2,0.102093900435219,0.26516250235706784,0.49,0.75,1.2,1.7]
[null,null,null,null,null,null,null,null,6,3,3.25702788673096E-2,8.1253736839137683E-2,0.20944703712179186,0.36738226990392298,0.5400613050103229,0.89238932220585143,1.3508024954966302]
[null,null,null,null,null,null,null,null,7,3.5,2.1228098201979011E-2,5.7259558218632524E-2,0.15760651502849371,0.28495903112470816,0.43923123183947704,0.76360563474177001,1.1492298511427237]
[null,null,null,null,null,null,null,null,8,4,1.1931947635136943E-2,3.4288708671029282E-2,0.10320863945494078,0.21083014742978995,0.33355571788832256,0.60272479516716071,0.92116043701840089]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)",null,null,null,null,null,null,9,4.5,8.1275568607984197E-3,1.8414098276976709E-2,6.3162670572028137E-2,0.13218463197550756,0.22563854312247,0.45819301177171112,0.69670682808105178]
["Cetnost opakování:","N=",2,"(let)",null,null,null,null,10,5,2.2637775422077945E-3,1.2343680860319223E-2,4.210085731645706E-2,7.2155549005529451E-2,0.14280910455987794,0.29179525001458295,0.47860846923316802]
["Hodnota kulminace (dle CHMU):","Qmax=",0.14000000000000001,"(m3/s)",null,null,null,null,11,5.5,1.5239169113996968E-3,3.4526434269331625E-3,2.0407572263646801E-2,6.5999235686809141E-2,9.7635771384257122E-2,0.17553685186888723,0.31422509332848914]
["Poradnice doby kulminace","IMAX=",4,"(-)",null,null,null,null,12,6,1.5239169113996968E-3,3.4526434269330948E-3,7.8939107468357309E-3,1.2959328430198964E-2,5.9808598711358768E-2,0.15318158508116689,0.22049746493474787]
["Doba dobihani:","TL=",1.5950505562267492,"(hod)",null,null,null,null,13,6.5,1.5239169113996968E-3,3.4526434269331625E-3,7.8939107468357309E-3,1.2959328430198964E-2,1.8306707134548128E-2,6.5402481537756366E-2,0.16325774552028058]
["Objem vlny:","VOL=",1.1007881294945352,"(tis. m3)",null,null,null,null,14,7,1.5239169113996968E-3,3.4526434269330948E-3,7.8939107468355627E-3,1.2959328430199254E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675264691E-2]
[null,null,null,null,null,null,null,null,15,7.5,1.5239169113997252E-3,3.4526434269330948E-3,7.8939107468357309E-3,1.2959328430198964E-2,1.8306707134548128E-2,2.8721547202718065E-2,4.1343274675265766E-2]
[null,null,null,null,null,null,null,null,16,8,1.5239169113996968E-3,3.4526434269331625E-3,7.8939107468357309E-3,1.2959328430198964E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675264691E-2]
[null,null,null,null,null,null,null,null,17,8.5,1.5239169113996968E-3,3.4526434269330948E-3,7.8939107468357309E-3,1.2959328430198964E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675265766E-2]
[null,null,null,null,null,null,null,null,18,9,7.972380278306497E-4,3.4526434269331625E-3,7.8939107468355627E-3,1.2959328430199254E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675264691E-2]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)",null,null,null,null,null,null,19,9.5,null,1.5554350683595077E-3,7.8939107468357309E-3,1.2959328430198964E-2,1.8306707134548128E-2,2.8721547202718065E-2,4.1343274675265766E-2]
["Cetnost opakování:","N=",5,"(let)",null,null,null,null,20,10,null,null,7.3750717922329246E-3,1.2959328430198964E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675264691E-2]
["Hodnota kulminace (dle CHMU):","Qmax=",0.3,"(m3/s)",null,null,null,null,21,10.5,null,null,null,1.2959328430198964E-2,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675265766E-2]
["Poradnice doby kulminace","IMAX=",4,"(-)",null,null,null,null,22,11,null,null,null,6.1037777287657833E-4,1.8306707134548128E-2,2.872154720271879E-2,4.1343274675264691E-2]
["Doba dobihani:","TL=",1.7434273521548187,"(hod)",null,null,null,null,23,11.5,null,null,null,null,2.9277085681673216E-3,2.8721547202718065E-2,4.1343274675265766E-2]
["Objem vlny:","VOL=",2.7191700169708883,"(tis. m3)",null,null,null,null,24,12,null,null,null,null,null,1.8487870939425877E-2,4.1343274675264691E-2]
[null,null,null,null,null,null,null,null,25,12.5,null,null,null,null,null,null,1.5941032331564693E-2]
[]
[]
[]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)"]
["Cetnost opakování:","N=",10,"(let)"]
["Hodnota kulminace (dle CHMU):","Qmax=",0.49,"(m3/s)"]
["Poradnice doby kulminace","IMAX=",5,"(-)"]
["Doba dobihani:","TL=",1.8547099491008712,"(hod)"]
["Objem vlny:","VOL=",4.7132284286659427,"(tis. m3)"]
[]
[]
[]
[]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)"]
["Cetnost opakování:","N=",20,"(let)"]
["Hodnota kulminace (dle CHMU):","Qmax=",0.75,"(m3/s)"]
["Poradnice doby kulminace","IMAX=",5,"(-)"]
["Doba dobihani:","TL=",1.9659925460469236,"(hod)"]
["Objem vlny:","VOL=",7.0100685883277807,"(tis. m3)"]
[]
[]
[]
[]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)"]
["Cetnost opakování:","N=",50,"(let)"]
["Hodnota kulminace (dle CHMU):","Qmax=",1.2,"(m3/s)"]
["Poradnice doby kulminace","IMAX=",5,"(-)"]
["Doba dobihani:","TL=",2.1143693419749932,"(hod)"]
["Objem vlny:","VOL=",11.734562130081802,"(tis. m3)"]
[]
[]
[]
[]
["Vystup procedury Flood_V:","Výsledné hydrogramy (proporcionální s TUH_SCS)"]
["Cetnost opakování:","N=",100,"(let)"]
["Hodnota kulminace (dle CHMU):","Qmax=",1.7,"(m3/s)"]
["Poradnice doby kulminace","IMAX=",5,"(-)"]
["Doba dobihani:","TL=",2.1885577399390277,"(hod)"]
["Objem vlny:","VOL=",17.421343912015477,"(tis. m3)"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}